How to Change MAC Address (Using T-MAC)

1. Starting MAC address changer will list all available network adapters.
2. Select the adapter you want to change the MAC address of. You will get the details of your selection below.
3. In the **Information** tab, find the **Change MAC Address** frame. Enter new MAC address in the field and click **Change Now!** button. You may even click the **Random MAC Address** button to fill up a randomly selected MAC address from the vendor list available.
4. To restore the original MAC address of the network adapter, select the adapter, click **Restore Original** button in the **Change MAC Address** frame.

**NOTE:** This tool **cannot** change MAC address of **Microsoft Network Bridge**. Network Bridge **will automatically use the original MAC address** of the **first NIC added into bridge** with **the first octet of MAC address set to 0x02**.